XMI DRAIN STRIKE — SPEC SUMMARY

Series Overview
- Volt Series (Blue): Electric / zero-emission sewer and drain jetter
- HD Series (Green): Diesel / long-run production sewer and drain jetter
- Pro Series (Red): Gas + hot water / grease-clearing sewer and drain jetter

Volt Series — DS-30Ke
- Power: 22KW electric
- Pressure: 2,900 PSI
- Flow: 9.3 GPM
- Best fit: low-noise sites, sensitive properties, indoor-adjacent jobs

HD Series — DS-300HDE
- Power: 65HP diesel
- Pressure: 4,350 PSI
- Flow: 18.5 GPM
- Tank: 158 gallons onboard
- Best fit: contractor and municipal production work, remote or high-output jobs

Pro Series — DS-300HWE
- Power: 40HP gas
- Pressure: 4,350 PSI
- Flow: 13.2 GPM
- Heating: 13 gallons, up to 194°F
- Best fit: grease-heavy commercial drains, kitchens, restaurants, food service work

Positioning
- Three job-specific builds on one platform
- Built for contractor, fleet, and municipal quoting conversations
